|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  |  |  | | --- | --- | --- | | **U-9: FISHERMAN’S HANGING LIGHT**   |  |  | | --- | --- | |  |  |   UL basic mark listed ;Interior / Exterior (Covered) Residential & Commercial Use  Max Wattage:  100w LED Equivalent; 75w Incandescent Bulb ;  Medium Base (E26) Socket, Dimmable (GU-24 also available)  Glass: Frosted Glass Only    Mounting: 4.8” Mounting back plate attaches to standard box. 20” of chain is provided, more available upon Request. All Install Hardware Provided.    Options: Pole Mounted Version (U-9TUB) Available    Material: Solid Brass Construction | | **Available Finishes**   |  |  | | --- | --- | | Standard Finishes:    Unlacquered Brass – $655    Lacquered Brass - $655  *Typically in-stock & available for immediate shipment* | Custom Finishes\*: $855 Each  Brass (Antique, Lacquered, Satin)  Copper (Antique, Polished, Satin)  Nickel (Antique, Polished, Satin)  Oil Rubbed Bronze ~ Pewter  Polished & Satin Chrome ~ Verdigris  Powder Coat (All Colors Available)  Custom Matching Also Available    *\*Custom Finish Info: 4-8 weeks unless in-stock; Rush Available; Special Orders not Refundable; Custom Lights often in-stock ; Minimum of two lights if not in-stock* |  |  |  | | --- | --- | |  | 68 Front St. Marblehead, MA 01945  p. 781-631-3864 f. 781-823-5555 info@shiplights.com  *~ A Division of Brass ‘N Bounty~* | | |

SOLID BRASS ~ WEATHER-PROOF ~ UL LISTED ~ DURABLE