|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |

|  |  |  |
| --- | --- | --- |
| **U-9: FISHERMAN’S HANGING LIGHT**

|  |  |
| --- | --- |
|  |  |

UL basic mark listed ;Interior / Exterior (Covered) Residential & Commercial UseMax Wattage: 100w LED Equivalent; 75w Incandescent Bulb ; Medium Base (E26) Socket, Dimmable (GU-24 also available) Glass: Frosted Glass Only  Mounting: 4.8” Mounting back plate attaches to standard box. 20” of chain is provided, more available upon Request. All Install Hardware Provided. Options: Pole Mounted Version (U-9TUB) Available  Material: Solid Brass Construction   |
| **Available Finishes**

|  |  |
| --- | --- |
| Standard Finishes: Unlacquered Brass – $655 Lacquered Brass - $655*Typically in-stock & available for immediate shipment* | Custom Finishes\*: $855 EachBrass (Antique, Lacquered, Satin)Copper (Antique, Polished, Satin)Nickel (Antique, Polished, Satin)Oil Rubbed Bronze ~ PewterPolished & Satin Chrome ~ VerdigrisPowder Coat (All Colors Available)Custom Matching Also Available *\*Custom Finish Info: 4-8 weeks unless in-stock; Rush Available; Special Orders not Refundable; Custom Lights often in-stock ; Minimum of two lights if not in-stock* |

|  |  |
| --- | --- |
|  | 68 Front St. Marblehead, MA 01945 p. 781-631-3864 f. 781-823-5555 info@shiplights.com*~ A Division of Brass ‘N Bounty~* |

 |

 |

SOLID BRASS ~ WEATHER-PROOF ~ UL LISTED ~ DURABLE